Joy Button, ESP32 Edition

# SD

# MP3

# LCD with I2C

The ESP32 has two I2C channels and any pin can be set as SDA or SCL. When using the ESP32 with the Arduino IDE, the default I2C pins are:

* GPIO 21 (SDA)
* GPIO 22 (SCL)

# Rotary Encoder

All pins can be enabled as interrupts! <https://randomnerdtutorials.com/esp32-pir-motion-sensor-interrupts-timers/>